	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-061L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 500
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 13
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 160
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		58
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		6
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3.5
14	LOCATION			BHP RATED (kW)		0.028
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS63K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		20	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-062L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 500
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 26
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 160
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		116
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		6
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3.5
14	LOCATION			BHP RATED (kW)		0.046
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS63K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		20	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-121L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 500
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 55
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 160
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		58
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		12
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3.5
14	LOCATION			BHP RATED (kW)		0.085
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS63K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		20	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-122L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 500
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 110
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 160
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		116
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		12
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3.5
14	LOCATION			BHP RATED (kW)		0.133
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS63K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		20	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-161L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 1000
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 100
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 160
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		58
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		16
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3
14	LOCATION			BHP RATED (kW)		0.118
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS63K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		21	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-162L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 1000
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 205
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 100
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		116
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		16
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3
14	LOCATION			BHP RATED (kW)		0.144
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS63K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		21	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-221L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 1000
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 195
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 104
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		58
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		22
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3
14	LOCATION			BHP RATED (kW)		0.146
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS40K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		21	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-222L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 1000
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 400
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 52
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		116
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		22
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3
14	LOCATION			BHP RATED (kW)		0.141
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS40K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		21	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-301L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 1000
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 350
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 56
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		58
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		30
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3
14	LOCATION			BHP RATED (kW)		0.146
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS20K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		22	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.

	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-302L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 1000
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 740
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 28
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		116
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		30
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3
14	LOCATION			BHP RATED (kW)		0.141
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS20K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS20K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1700
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		B
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP44
31	WEIGHTS (kg)		22	HUB SIZE		Ø21
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.